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· 4 Megapixel CMOS Sensor
· Onvif Profile S Compliant
· 3-Axis adjustment
· 2.8-12mm Motorised Lens
· 3D Digital Noise Reduction
· Digital Wide Dynamic Range
· Power over Ethernet
· 20-30m IR LED
· True Day/Night IR Cut Filter
· H.265 / H.264 Compression
· Dual Streaming
· Micro-SD Card Slot
· Grey or White Housing

PRIME IP4-EEDI2812MG/W
External Eyeball Dome with Motorised Zoom Lens (4MP)

 (
Hardware
Image Sensor
1/3” Sony Exmor CMOS
Electronic Shutter
1/25s ~ 1/10000s
Sensitivity
0 Lux (IR On)
0.5 Lux Colour / 0.2 Lux B/W
Lens Type
2.8 - 12mm Motorised AF Lens
Lens Interface
M12
ICR
Mechanical IR cut filter
LED
2 Hi-Intensity IR LED
20-30m
 
Distance
 
(scene
 
dependent)
Alarm I/O
No
PoE
Yes, (IEEE802.3af)
Connections
12VDC, RJ45 Network
Power
PoE 802.3af / 12VDC 
5.5W
 
(IR
 
Off),
 
7W
 
(IR
 
On)
Operating Temperature
-10ºC ~ 50ºC IP65 Rated
Dimensions
ø120mm x 95mm (H)
Weight
680g
) (
System
Video Resolution 
options
2592 x 1520 @ 20pps
At
 
25pps:
 
2560
 
x
 
1440,
 
1080P, 
720P,
 
D1,
 
VGA,
 
2CIF,
 
CIF,
 
QCIF
Video Adjustment
 
options
Brightness, Contrast,
 
Saturation, Sharpness,
 
AGC,
 
WDR,
 
Mirror,
 
3D 
Noise reduction,
 
Defog
Dual Streaming
Yes
Image Snapshot
Yes
Privacy Mask
Yes - 4 zones
Compression Format
H.265 / H.264 / MJPEG
Video Bitrate range
16Kbps ~ 8Mbps
Onboard Storage
Micro-SD Card Slot
Video Bitrate Encoding
CBR, VBR
Motion Detection
Yes - Multi level sensitivity
OSD
Time/Date, Title
Alarm Functions
Video Loss, Network, Tampering, 
Motion Detection, ROI
Trigger Actions
Email, Snapshot, Zoom Preset
Security
Password
Firmware Upgrade
Yes, possible remotely via browser
)Technical Specification



	Network

	Ethernet
	10/100 Base-T
RJ45 cable connection

	Network Protocols
	TCP/IP, UDP, HTTP, DHCP, NTP, RTSP, PPPoE, DDNS, SMTP, UPNP, FTP
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